## Comms Configurator config file for the BServer
## size in bytes
## 16000, 16KB NOT enough
## 160000, 160KB NOT enough
## 1600000, 1.60MB 	(OK,1362MB, 1362224 left)
## 300000, 0.30MB	(OK, 70	MB,   70804 left)
## 500000, 0.50MB 	(OK, 272MB,  271584 left)

[Loader]
Name=CBridgeServer
FileName=BServer.dll
IsServer=1
IsSticky=1
Priority=EPriorityNormal
StackSize=8000
ScaledStartupState=0x1050
HeapOption=ENewHeap
MinHeapSize=500000
MaxHeapSize=800000
SystemCritical=1
ControlFlags=1


