#
# BT Factory Settings Information File
# ====================================
#
# All Factory settings information must be stored as follows
#
# Philips:
# <CHIP_ID> <HCI_revision> <LMP_Subversion> <FactorysettingsFile_HEAD_xx)>
#
# there CHIP_ID, HCI_revision and LMP_Subversion are read from firmware at start-up.
#
# ST: <CHIP_ID> is set to 0x00000000 since this is not used by ST.
#
# NOTE: From STE platform P1T and later <CHIP_ID> information shall not be listed!
#
# ====================================
# STLC2500_R4_02_05.ssf                                                          static settings file for STLC2590 and 2500C4 (minikit)
# STLC2592_R5_01_02_UART.ssf                                                     static settings file for STLC2592   (minikit)
# STLC2593_R5_02_01_UART.ssf                                                     static settings file for STLC2593 D2 (minikit)
# STLC2593_R5_03_05_SEMC_SPI_unified_Lisbon.ssf                                  static settings file for STLC2593 D3, Lisbon enabled
# STLC2594_R5_04_02_SEMC_SPI.ssf                                                 static settings file for STLC2593 D4
# STLC2500_R6_00_01_SPI_SEMC_Maxipard.ssf                                        static settings file for STLC2690 CUT 1 (used in Maxipard)
# STLC2600_R6_03_02_E1_SPI_SEMC.ssf                                              static settings file for STLC2690 CUT 2.1 (used in Susan PDP)
# STLC2600_R6_04_03_SEMC-GPIO12-13_nobla.ssf                                     static settings file for STLC2690 CUT 3.0 CB10EG (LMP_Subversion 1D)
# STLC2600_R6_04_03_SEMC-GPIO12-13_nobla.ssf                                     static settings file for STLC2690 CUT 3.0 CB10EH (LMP_Subversion 1E)
# STLC2600_R6_05_03_SEMC.ssf                                                     static settings file for STLC2690 CUT 4.0 (LMP_Subversion 1F)
# STLC2600_R6_05_11_SEMC.ssf                                                     static settings file for STLC2690 CUT 4.1 (LMP_Subversion 2F)
# ----------------------------------------------------------------------------------------
0x0402  0x0520  STLC2500_R4_02_05.ssf
0x0501  0x00EF  STLC2592_R5_01_02_UART.ssf
0x0502  0x00F0  STLC2593_R5_02_01_UART.ssf
0x0503  0x00F1  STLC2593_R5_03_05_SEMC_SPI_unified_Lisbon.ssf
0x0504  0x00F2  STLC2594_R5_04_02_SEMC_SPI.ssf
0x0600  0x0001  STLC2500_R6_00_01_SPI_SEMC_Maxipard.ssf
0x0603  0x0014  STLC2600_R6_03_02_E1_SPI_SEMC.ssf
0x0604  0x001D  STLC2600_R6_04_03_SEMC-GPIO12-13_nobla.ssf
0x0604  0x001E  STLC2600_R6_04_03_SEMC-GPIO12-13_nobla.ssf
0x0605  0x001F  STLC2600_R6_05_03_SEMC.ssf
0x0605  0x002F  STLC2600_R6_05_11_SEMC.ssf
