Mini SuperMode for VGA CAM
Features:

-Manual settings:Photo/Video
-Exposure EV
-Shutter Speed:ISO(Shutter Delay+Shutter Width)/Sharpness
-Saturation/Effects
-Contrast/ Brightness
-White Balance/Color Correction

How to upload camdriver0.dat and *.lng to phone:
- download XS++ 3.1.(example programm phone xs++)
- shut down your phone.
- run XS++, click on 'Connect', put USB cable to your PC, while pressing 'C' key on your phone, put the other side of cable to your phone, wait XS++ recognize your phone.
- click on FSX™ radio button, click on 'Start FSX', wait a minute or two.
- find IFS/SETTINGS/CAMERA, drag and drop camdriver0.dat to right window.
- find TPA/PRESET/SYSTEM/LANGUAGE, drag and drop *.lng to right window.
- in XS++ click on 'Shutdown', then click on 'Yes'.
- close XS++ and disconnect your phone.

Download setool (example programm setool)

How to Proceed in CID 50/51/52 with the program *SETOOL/PHONEXS++/FAR:

*SETOOL USER GUIDE

1-Unpack the folder tpa_ifs

2-Copy in its tpa_ifs this way: ifs/settings/camera

3-Copy the file "camdriver0" the latest version to the place indicated

4-After passing your tpa_ifs compressed in *.Zip by SETOOL

5-Press the button Flash

6- find TPA/PRESET/SYSTEM/LANGUAGE in MISC FILES click in FLASH botton

7-Wait finish the process with the message ready

How to use this camdriver: MiniSuperMode for VGA CAM

- Changing Exposure EV: in menu choose Manual settings, choose Exposure, with joypad you can change its value

Value | -2.0 | -1.7 | -1.3 | -1.0 | -0.7 | -0.3 | 0.0 | +0.3 | +0.7 | +1.0 | +1.3 | +1.7 | +2.0
Equivalent EV | 100% | 85% | 75% | 50% | 25% | 15% | 0% | 15% | 25% | 50% | 75% | 85% | 100%

- Changing Shutter Speed: in menu choose Manual settings, choose Shutter Speed:ISO/Sharpness, with joypad you can change its value.

Value | 0.0 | +0.3 | +0.7 | +1.0 | +1.3 | +1.7 | +2.0
Equivalent ISO/Shutter Speed | Auto Default | ISO100/7.5FPS | ISO125/10FPS | ISO160/14FPS | ISO200/15FPS | ISO320/25FPS | ISO500/30FPS

- Changing Sharpness: in menu choose Manual settings, choose Shutter Speed:ISO/Sharpness, with joypad you can change its value.

Value | -2.0 | -1.7 | -1.3 | -1.0 | -0.7 | -0.3 | 0.0
Equivalent Sharpness | +1 Min | +2 | +3 | +4 | +5 | +6 Max | Auto

- Changing Saturationand Effects: in menu choose Manual settings, choose Saturation with joypad you can change its value.

Value | 0.0 | +0.3 | +0.7 | +1.0 | +1.3 | +1.7 | +2.0
Equivalent Saturation | 0% | 15% | 25% | 37.5% | 60% | 85% | 100% full saturation

- Changing Saturarion and Effects: in menu choose Manual settings, choose Effects with joypad you can change its value.

Value | -0.3 | -0.7 | -1.0 | -1.3 | -1.7 | -2.0 | 0.0
Equivalent Sharpness | Black and White | Sepia | Solarize | Negative | Normal | Normal | auto

- Changing Brightnesst: in menu choose Manualsettings, choose Contrast/ Brightness, with joypad you can change its value.

Value | -2.0 | -1.7 | -1.3 | -1.0 | -0.7 | -0.3 | 0.0
Equivalent Brightness | 15% | 25% | 35% | 50% | 85% | 100% full | 0

- Changing Contrast: in menu choose Manualsettings, choose Contrast/Brightness ,with joypad you can change its value.

Value | 0.0 | +0.3 | +0.7 | +1.0 | +1.3 | +1.7 | +2.0
Equivalent Contrast | 0 | 15% | 25% | 50% | 75% | 85% | 100%

- Changing White Balance: in menu choose Manualsettings, choose White Balance/Color Correction,with joypad you can change its value. White Balance is relative to current white balance.

Value | 0.0 | +0.3 | +0.7 | +1.0 | +1.3 | +1.7 | +2.0
Equivalent White Balance | Auto | Normal | Incandescent (Tungsten) | Fluorescent (white ice or yellow ligth) | Clear Sky | Cloudy | Effect Luminosity

- Changing Color Correction: inmenu choose Manual settings, choose White Balance/Color Correction,with joypad you can change its value. Color Correction is relative to current color correction.

Value | -2.0 | -1.7 | -1.3 | -1.0 | -0.7 | -0.3 | 0.0
Equivalent Effects | Color Correction Blue high | Color Correction Blue low | Color Correction Green high | Color Correction Green low | Color Correction Red high | Color Correction Red low | Auto

BrAzzUkA´s

Thanks to friends and developers

Alex Herdea Daniel Vlad Sadeghi SPU, Raiderski, Sadeghi, Sergiober and the others modders developers

Visit website:

http://www.esato.com/board/viewtopic.php?topic=159467&start=0

Guide User Language Mini SuperMode VGA CAM

-Changes version for Mini SuperMode for VGA CAM:

Effects | => | Manual Settings
Off | => | Exposure
Black&White | => | White Balance/Color Correction RGB
Negative | => | Saturation / Effects
Sepia | => | Contrast/ Brightness
Solarize | => | Shutter Speed:ISO/Sharpness

-Mudanças versão para Mini SuperMode para VGA CAM:

Efeitos | => | Manual Configurações
Desativar | => | Exposição
Branco e Negro | => | Equilíbrio de Branco/Correção Cor
Negativo | => | Saturação / Efeitos
Sepia | => | Contraste/Brilho
Clarear | => | Disparo obturador:ISO/Nitidez

Based on firmware w200 CID52-R4HA014

Baseado no firmware w200 CID52-R4HA014

Table Manual Settings MiniSuperMode VGA CAM

Joypad(+/-) | Exposure EV | Contrast/ Brightness | Saturation/Efeitos | White Balance/Color Correction | Shutter Speed:ISO/ Sharpness
2,0 | EV+2,0 | 100% | 100% | Effect Luminosity | ISO500-30FPS
1,7 | EV+1,7 | 85% | 85% | Cloudy | ISO320-25FPS
1.3 | EV+1,3 | 75% | 60% | Clear Sky | ISO200-15FPS
1,0 | EV+1,0 | 50% | 37,5% | Fluorescent (white ice or yellow ligth) | ISO160-14FPS
0.7 | EV+0,7 | 25% | 25% | Incandescent (Tungsten) | ISO125-10FPS
0,3 | EV+0,3 | 15% | 15% | Auto normal | ISO100-7.5FPS
0.0 | AUTO | AUTO | AUTO | AUTO | AUTO
-0,3 | EV-0,3 | 100% | Black&White | Color Correction red low | +6 MAX
-0,7 | EV-0,7 | 85% | Sepia | Color Correction red high | +5
-1,0 | EV-1,0 | 50% | Negative | Color Correction green low | +4
-1,3 | EV-1,3 | 35% | Solarize | Color Correction green high | +3
-1,7 | EV-1,7 | 25% | OFF NORMAL | Color Correction blue low | +2
-2,0 | EV-2,0 | 15% | OFF NORMAL | Color Correction blue high | +1 MIN

BrAzzUkA´s

Visit website:

http://www.esato.com/board/viewtopic.php?topic=159467&start=0