//########################################################################################################
//#  ____                      _____      _                                                              #
//# / ___|  ___  _ __  _   _  | ____|_ __(_) ___ ___ ___  ___  _ __                                      #
//# \___ \ / _ \| '_ \| | | | |  _| | '__| |/ __/ __/ __|/ _ \| '_ \                                     #
//#  ___) | (_) | | | | |_| | | |___| |  | | (__\__ \__ \ (_) | | | |                                    #
//# |____/ \___/|_| |_|\__, | |_____|_|  |_|\___|___/___/\___/|_| |_|                                    #
//#                    |___/                                                                             #
//#                                                                                                      #
//# Version v3.0 Extreme Sharpness™ Special Edition BrAzzUkA's Team BZK®                                 #
//# Optimized for the Sony Ericsson w995                                                                 # 
//########################################################################################################
//# Copyright® 2009 Sony Ericsson Mobile Communications.                                                 #
//# All rights, including trade secret rights, reserved.                                                 #
//# BrAzzUkA's Team BZK® Camera Drivers respects the intellectual property of others,                    #          
//# and we ask our modders and users to do the same.                                                     #
//########################################################################################################
Visit the website: 
http://forums.se-nse.net/index.php?showtopic=43199&hl=camdriver%20w995&st=0
http://www.esato.com/board/viewtopic.php?topic=191301

You "User" please First read this before any movement:

Only advanced users and modders.
User If you don´t know or don´t want to change anything in your driver doesn´t edit and not touch anything below

To take good photos you must first use the resources of your camera. The AUTO mode is the scene of the mobile phone standard, one that fits
by default in every kind of situation, so she must have median values of ISO, and shots etc. .. So, use all resources possible that your camera offers for
get a good picture.

==========================================================
Changelog:v3.0_Extreme Sharpness™ Special Edition_for_w995
==========================================================

USER GUIDE MANUAL v3.0_Extreme Sharpness™ Special Edition_for_w995:

-Removed some lines of property FLASH_SETTINGS 
-Removed some unnecessary lines of code 
-Code clean and optimized
-Add the function iso manual photo mode and effects video mode in Flash support
-Decrease Master Clock™ to 13mhz 

About Led Flash:
-Removed Led flash forced any conditions luminosity
-Now added original led flash schema
-Removed led flash forced any conditions luminosity. Added original Led flash but manual shutter speed led flash continue working normally together with the driver optimized and others functions.

Colors correction WB RGB:

Led Flash On -> Color Correction WB RGB OFF!
Led Flash Off -> Color Correction WB RGB ON!
*colors correction WB RGB

Colors correction Led Flash (enable):

Led Flash On -> Color Correction Led Flash ON!
Led Flash Off -> Color Correction Led Flash OFF!
*colors correction only for led flash enable on

How to work colors corrections WB RGB and colors correction LED Flash???
The sensor provides two color corrections one color corrections WB RGB and other color corrections with led flash are two colors correction and distinct colors correction.
The color corrections are optimized to work separately not compromising the colors.

About Colors Correction:if necessary "user" you can change the values for the colors correction.
Look the table colors corrections below.

*WB= White Balance

Find this line in inside of camdriver0.dat and change the values always in numbers hexa.
=====================================
WB_CC =
	#SET_REG(66,yy) =>change (yy) if necessary
	#SET_REG(65,xx) =>change (xx) if necessary
	$p5 10
	$c5 00
		#COM_EVENT(58,XX) =>change (xx) if necessary
	$cl
		#COM_EVENT(58,XX) =>change (xx) if necessary
	$cx
	#COM_EVENT(13,01);

=====================================

Table Colors Corrections for w995:
---------------------------------

xx = 00 - 7F = cyan, 80 - FF = red
yy = 00 - 7F = yellow, 80 - FF = magenta 


======================================================================

Led Flash:

-Led flash turn on only in condition stable of luminosity
-Led flash with High light turn off [enable]
-Led flash with Low light turn on [enable]

About Colors Correction works together with Led Flash:
-Led Flash turn on [enable] in your w995 the colors correction off [disable]
-Led Flash turn off [disable] in your w995 the colors correction on [enable] 

======================================================================
Video:

Now you can have a full features for your w995 "user" so start with iso manual for photos and effects for video enjoy!

Two [2] Resolutions for video recording Two [2] Movie Size

Movie Size: 
-320x240 Normal video recording 25fps to 30fps [QVGA] 
-VGA 640x480 video recording 12fps to 15fps [VGA] (synchronized to better performance of video) or
-CIF 352x288 video recording 15fps to 25fps 
Access the Menu Mode Night or Mode Video:
-To video recording in normal video resolution 320x240 , just switch to video mode Normal Mode (disable Nigth Mode) or Normal resolution 320x240.
-To video recording in VGA resolution 640x480 or CIF resolution 352x288 , turn Nigth Mode or VGA resolution 640x480/CIF resolution 352x288. 
The new built-in video camera w995 VGA 640x480 resolution or CIF 352x288 resolution is ready for anything. 
Now included and implemented Special effects working normally with your video and enjoy with focus manual. 
Five video effects default let you add to your video. 
Youtube: Syncronize your w995 video and Share with your friends or put more you in YouTube in VGA 640x480 resolution.It’s just as easy Syncronize on a PC when you use your favorite photo software and the video file sizes are perfect for sharing on YouTube or emailing to friends. 

*Use the graphical interface *LNG for greater convenience for Mode Video

Attention:Yet w995 VGA 640x480 video recording is subject some bugs by the limited hardware sometimes appear a few green lines in video recording but nothing that we are compromising their performance. 
Another inconvenience you can not watch the videos recorded in VGA mode in your W995 can only watch the videos on your PC by limited hardware.

Photos: ISO MANUAL (*Special Controllers Särskilda Kontrollerkort)

//==========================ISO MANUAL
// Property 8, Effects=ISO MANUAL
0 => normal = ISO Auto,
1 => negative = ISO 100
2 => solarize = ISO 200
3 => sepia = ISO 400
4 => black&white = ISO 800
//==========================ISO MANUAL 

Video: EFFECTS (*Special Controllers Särskilda Kontrollerkort)

//==========================EFFECTS
// Property 8, Effects
0 => normal 
1 => negative 
2 => solarize 
3 => sepia 
4 => black&white 
//==========================EFFECTS

*Special Controllers Photo/Video Särskilda Kontrollerkort Foto / Video:
-Photo Mode: original EV
-Video Mode manual focus 
-Now you "user" have two user controls in your hands:Video mode using the manual focus can work with all the effects available and another way to Photo mode using original ev controlling the basic functions.
-Nu har du två användare kontroller i händerna: Video, med användning av manuell fokusering kan arbeta med alla de effekter som finns tillgängliga och en annan väg till Photo-läge med original ev styra grundläggande funktioner

======================================================================
Scenes:

-Night Scene

Shooting in 1 seconds shutter speed 1s

Video: 

Now two resolutions video recording w995.Access the Menu Mode Night or Mode Video

-Normal Video Recording 320x480 resolution

-VGA Video Recording 640x480 resolution or VGA Video Recoding 352x288 resolution

Video Capture

-Now VGA video, 640 by 480 pixels, 12fps to 15fps frames per second condition luminosity
-Now CIF video, 352 by 288 pixels, 15fps to 25fps frames per second condition luminosity
-5 real time effects:normal, negative, solarize, sepia, black&white
-Now Video mode with focus manual

*Attention:VGA video recording 640x480 by the limited hardware sometimes appear a few green lines in video recording but nothing that we are compromising their performance. 

===============================================================================================================================================================================
Instructions:
===============================================================================================================================================================================
The driver must be installed in this folder:

IFS \ SETTINGS \ CAMERA

Delete the file "camdriver0.dat" and "camdriver1.dat" and drag and drop the file Unpack with the same names (CAN NOT BE DIFFERENT NAME).

camdriver0.dat=> for camera
camdriver1.dat=> for frontal camera or video call

Files *. lng (language)
Should be placed in this folder:

TPA \ PRESET \ SYSTEM \ LANGUAGE

Drag and drop the files "pb.lng" and "en.lng" "de.lng" "sv.lng" folder above.




Visit website:
http://forums.se-nse.net/index.php?showtopic=43199&hl=camdriver%20w995&st=0
http://www.esato.com/board/viewtopic.php?topic=191301

//   ########                    #####
//  ###########              ####     ##
//   ###########           ###        # 
//   #############        ##            
//   ##############     ##              
//   ###############   ##               
//    ############### ##                
//     ################                 
//         #        ############        
//      #           ###############     
//     #           #################    
//     #          ##################    
//     ##         ##  ##############    
//      #  ©2010 ##    ###BZK®™#####    
//       ##  #  ##      ##########      
//         #####          ######
// Sony Ericsson CameraDrivers BrAzzUkA's Team BZK®
//
//Programming Software Sensor Camera License Agreement:
//The CameraDrivers BrAzzUkA's Team BZK® grants you a limited licence to use the codes of the sensors camera and the codes of the sensors second camera embedded in this driver "the Software" in binary and hexadecimal executable form in the normal operation of the driver. Title ownership rights and intellectual property rights and Logic Programming and Programming Sensors remain in CameraDrivers BrAzzUkA's Team BZK®.
//You acknowledge that Logic Programming and Programming Sensors is the property of CameraDrivers BrAzzUkA's Team BZK® and the codes of sensors is property Sony Ericsson and partner companies in the manufacture of sensors is protected under the Software License Agreement copyright laws and international copyright treaties. You further acknowledge that the structure, organization and codes programming sensors are avaliable trade secrets of CameraDrivers BrAzzUkA's Team BZK®.
//You agree not to decompile, disassemble, modifiy,reverse assemble, reverse engineer or reduce to human readable form the programming or any part of scheme or any part thereof or create any derivative works based on the programmin sensor or scheme CameraDrivers BrAzzUkA's Team BZK®.
//You agree not to export or re export, not copy or edit the programming sensor and schemma to any country or other vehicle communication in violation of the export control laws International.You agree not to sell the programming of sensor camera and the drivers in any hypothesis, that you and is explicit which may in no circumstances shall the sale of the drivers for profit under the law as the copyright.
//The information and codes published in camdrivers are available to any modders and user, 
//but may not necessarily be copied, downloaded or reused,reproduced without credit to the developers.
//Thanks and respect the developers. :)