- Register
- Help
- Remember Me?

1. If this is your first visit, be sure to check out the FAQ by clicking the link above. You may have to register before you can post: click the register link above to proceed. To start viewing messages, select the forum that you want to visit from the selection below.

Page 17 of 31 First ... 7 15 16 17 18 19 27 ... Last

- Jump to page:

Results 161 to 170 of 303

# Thread: UPDATES AND NEWS

- ###### Thread Tools

  - Show Printable Version

- ###### Display

  - Linear Mode
  - Switch to Hybrid Mode
  - Switch to Threaded Mode

1. 02-05-2010, 11:50 AM #161
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v0.915050
   > Saturday, 19 September 2009
   > - added alternative security bypass for semc a2 cid53 phones.
   > that allow you to repair completely dead a2 cid53 phones:
   > - destroyed trim area
   > - foreign gdfs
   > - damaged semcboot
   > please note, that alternative security bypass for a2 cid53 IS NOT free and NOT STANDALONE (check prices for details)
   > please note, that if you will execute alternative bypass mode for a2 cid53 in order to unlock/flash/etc - you will lose device key and drm functions possible will be damaged.
   > usage of a2 cid53 alternative security bypass exactly same as for a2 cid49/52 and explained in details in FAQ.
   > Download v0.915050

2. 02-05-2010, 11:51 AM #162
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v0.915051
   > Monday, 28 September 2009
   > - added full support for upcoming semc db3350 phones. as there are no phones on market, we can not test it, so support for db3350 marked as HIGHLY EXPERIMENTAL.
   > flashing/gdfs/filesystem operations should work flawlessly. full unlock via signature and "alternative bypass mode" SHOULD work too, but that things are absolutely not tested, so MAKE GDFS BACKUP before doing full unlock and only touch alternative security bypass if you absolutely crazy in any case, if phone will be killed - i will repair it for sure... well, you have been warned.
   > please note, that alternative security bypass for a2 db3350 cid53 IS NOT free and NOT STANDALONE (check prices for details)
   > please note, that if you will execute alternative bypass mode for a2 cid53 in order to unlock/flash/etc - you will lose device key and drm functions possible will be damaged.
   > - in some VERY RARE cases lg db3200 phones became completely dead after unlock attempt or unlock/flashing procedure failed in start. that should be fixed now, at least i received many good reports.
   > Download v0.915051

3. 02-05-2010, 11:52 AM #163
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v0.915052
   > Thursday, 8 October 2009
   > - tested,fixed and apporved support for db3350 phones, thx to imobile
   > as my "dear friends" used to say: world first, genuine,blablabla,etc.
   > anyway, i'm sure everything works now for db3350 -
   > - full signature unlock
   > - altbypass mode
   > - flashing,filesystem,gdfs,trim area operations.
   > - regarding a2 cid53 phones:
   > use full signature unlock for FULLY GENUINE unlock.
   > it is fast and furious (tm)
   > use alternative bypass mode for completely damaged phones.
   > it is slower, but can fix any software problem.
   > in next 2-3 days i will release next version, which will not damage
   > device key in a2 cid53 phones when using alternative bypass mode.
   > (need to arrange reset station upgrade, that require some time)
   > in any way, i strongly recommend to use full signature unlock for
   > a1/a2 phones - it is absolutely genuine and can not tamper anything.
   > v0.915052

4. 02-05-2010, 11:52 AM #164
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v0.915053
   > Friday, 9 October 2009
   > - a2 cid53 alternative bypass will not damage device key anymore. because of that one more phone restart required, but who cares ?
   > - "unlock during flash" enabled for s1 phone patch unlock
   > - some not important fixups, thx to imobile for bugreports.
   > Download v0.915053

5. 02-05-2010, 11:52 AM #165
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v0.915056
   > Friday, 6 November 2009
   > - added full support for s1_open PDA phones (satio).
   > big thanks to: cowboy, hardstone, shadowman,kris.sg for testing, arash for logo.
   > notes:
   > in order to boot satio you MUST check "signed mode" read flash requires "signed mode" and "alternative bypass" checked. satio omap nand flash starts at 8000000
   > to execute network unlock/repair - check both "signed mode" and "perform full unlock" then press unlock
   > to reset user code - check only signed mode and press unlock if "unlock after flash" checked - user code will be reset after flashing.
   > to flash satio you must add zip package to firmware area. do not unzip it !!!! just add.
   > - added possibility of generating new password for account.
   > Download v0.915056

6. 02-05-2010, 11:53 AM #166
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v0.915057
   > Tuesday, 1 December 2009
   > - added support for repair dead db3200-based lg phones (gt505,etc)
   > procedure:
   > if /sys partition damaged
   > (you CAN'T read gdfs, eraseSecData errors)
   > add to firmware area gt505_syspart_fix.ssw
   > press flash
   > unlock phone
   > fullflash phone
   > if /drm partition damaged
   > (phone blinks on lg logo after /sys repair and you CAN read gdfs)
   > add to firmware area gt505_drm_fix.ssw
   > press flash
   > unlock phone
   > fullflash phone
   > - added support for repair semc a2 phones with flash cid>otp cid
   > procedure:
   > check "use signed mode",
   > "use alternative security bypass",
   > "use preloader security bypass"
   > press unlock
   > credits consumption same as a2 cid53 unlock feature.
   > Download V0.915057

7. 02-10-2010, 05:05 PM #167
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v0.915058
   > - added support for repair erom on semc new security locosto,neptune phones.
   > procedure:
   > 1. select correct model
   > 2. on settings check "signed mode"
   > 3. add erom to firmware tab.
   > if you have neptune based phone: 1207-7713_EROM_S1_NEPTUN_HS_SEMC_SIMLOCK_R7A024.sin
   > if you have locosto based phone, then select situable from:
   > J132_EROM_S1_LOCOSTO_HS_USB_R5A038_64k.sin
   > K330_T280_T270_EROM_S1_LOCOSTO_HS_R5A028.sin
   > R300_R306_T303_S1_LOCOSTO_HS_R5A031_128.SIN
   > T250_CXC1250616_EROM_S1_LOCOSTO_HS_R5A022.sin
   > Z250_Z320_EROM_S1_LOCOSTO_HS_R5A023.sin
   > 4.press recovery
   > procedure require internet connection and paid: locosto based - 1 credit, neptune based - 2 credits.
   > - added support for high speed usb flashing. flashing speed of semc a2 phones will be twice as usual.
   > - some bugs fixed, one was very important
   > Download V0.915058

8. 02-11-2010, 12:42 PM #168
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v0.915059
   > - broken db200x PDA support, fixed
   > - broken alternative bypass support, fixed
   > Download V0.915059

9. 02-11-2010, 04:21 PM #169
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > i need to post few words about high speed flashing.
   > 1. not all a2 phones support it, you will get errors: 3ee,3ed. in that case just disable high speed usb flashing on a2 tab.
   > 2. you need to attach phone to usb 2.0 capable controller.
   > 3. you need to use high quality usb cable, dcu60 is NOT recommended (but can work). dcu65 IS recommended.

10. 02-12-2010, 08:50 PM #170
    the_laser
    - View Profile
    - View Forum Posts
    - Private Message
    Administrator

    Join Date
      Feb 2010
    Posts
      18,774

    ##

    > v0.915060
    > - broken calypso lite support, fixed
    > - broken cid16,29,36 support, fixed
    > - further fixes for alternative bypass support
    > important information.
    > in order to use latest update and further versions, users must install latest semc usb flash driver, at least version 2.2.0.1.
    > you can find semc usb flash driver setup package in
    > drivers\usbflash_driver\ggsetup-2.2.0.x.exe
    > Download V0.915060

Page 17 of 31 First ... 7 15 16 17 18 19 27 ... Last

- Jump to page:

Quick Navigation News & Updates Top

- Site Areas
- Settings
- Private Messages
- Subscriptions
- Who's Online
- Search Forums
- Forums Home
- Forums
- SETool2 Official support (English)
  1. News & Updates
  2. F.A.Q.
- HMD Tool Official support (English)
  1. News & Updates
- Other
  1. Offtopic & Trash

« Previous Thread | Next Thread »

#### Tags for this Thread

news, setool

View Tag Cloud

#### Bookmarks

- Digg
- Google
- del.icio.us
- StumbleUpon

#### Posting Permissions

- You may not post new threads
- You may not post replies
- You may not post attachments
- You may not edit your posts

- BB code is On
- Smilies are On
- [IMG] code is On
- [VIDEO] code is On
- HTML code is Off

Forum Rules