- Register
- Help
- Remember Me?

1. If this is your first visit, be sure to check out the FAQ by clicking the link above. You may have to register before you can post: click the register link above to proceed. To start viewing messages, select the forum that you want to visit from the selection below.

Page 23 of 31 First ... 13 21 22 23 24 25 ... Last

- Jump to page:

Results 221 to 230 of 303

# Thread: UPDATES AND NEWS

- ###### Thread Tools

  - Show Printable Version

- ###### Display

  - Linear Mode
  - Switch to Hybrid Mode
  - Switch to Threaded Mode

1. 09-13-2011, 12:24 PM #221
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v1.1108
   > Code:

   >     -  from now on, unlock by altbypass method for qsd8250,msm7227 phones will also "unlock" semcboot.
   >     -  qsd8250,msm7227 phones with "unlocked" bootloader can flash custom firmwares now
   >     -  added few models to model list, so users don't get confused
   >     -  different bugfixes, some are important.

   > RapidShare Link

2. 09-24-2011, 05:21 PM #222
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > WARNING !!!
   > As there is too much "blocked" setool2 GEMALTO TOP cards,we investigated issue and found problem.
   > due to errors in controller firmware
   > ( or due to incompatibility between smartcard/controller firmware/motherboard usb controller )
   > all smartcard readers i know, which are based on CY7C63001 are failed to send long data packet to/from smartcard.
   > it happens on some systems only, it can happen not immediately, but on "affected" system it happens always, earlier or later.
   > due to that, smartcard will receive WRONG command and SETOOL2 WILL BE "BLOCKED".
   > THAT IS NOT RELATED TO "BLOCKED CARDMANAGER" ISSUE ( ERROR #6982 )
   > i can not find ANY solution to that problem, other than NOT using Cypress CY7C63001-based readers with setool2 cards.
   > here is few pictures of AFFECTED readers:
   > CY7C63001.jpg CY7C63001_MXKEY.jpg
   > you can also identify such reader by smartcard reader name and driver name:
   > Example.JPG
   > if you will use that readers, your setool2 smartcard WILL BE BLOCKED - and i will unblock such card ONLY ONCE.
   > my strong recommendation is use omnikey-based readers, like that:
   > omnikey_bottom.jpg omnikey_top.jpg
   > they are working 100% on any system.
   > of course, usage of latest setool2 version is ABSOLUTE requirement.

3. 10-25-2011, 12:35 PM #223
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v1.12
   > Code:

   >     -  added altbypass support for xperia arc_s model, in other words, phones with 8255T chipset fully supported.
   >     -  added resurrection support for s1 qualcomm-based phones with totally damaged security zone.
   >        resurrection procedure will be described in FAQ later,
   >        however, in short it is standard "recovery+write gdfs+unlocking" chain.

   >        7227,8250-based phones require special uart cables ( pinout included in docs ),
   >        however it is highly recommended to use special GPG cables
   >        8x55-based phones does not require any special cables.

   >        as side effect, imei change possible now for s1 qualcomm-based phones.
   >        for 7227,8250-based phones need select COM as interface, options are:
   >        ( signed mode, altbypass mode, do full unlock, allow to change imei when unlocking, use testpoint (gnd type) )
   >        for 8x50-based phones need select USB as interface, options are:
   >        ( signed mode, altbypass mode, do full unlock, allow to change imei when unlocking )

   >        cost of imei change 5 credits, please take in mind, that if you change imei, phone need to be unlocked,
   >        so add another 5 credits for unlock procedure.
   >        if you have calculated signature for some imei, then you can save 5 credits for unlocking ;)

   >     -  added few models to model list, so users don't get confused
   >     -  different bugfixes

   > RapidShare Link

4. 10-26-2011, 12:35 PM #224
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v1.1201
   > Code:

   >     -  resurrection procedure will now work for totally erased s1 qualcomm-based phones
   >        FAQ now have  resurrection procedure example.

   >     -  forgot to post, that starting from v1.12 setool2 will check for faulty cypress-based reader and refuse to run,
   >        if setool2 smartcard installed in such reader.
   >        There is no any workaround.
   >        Use omnikey-based reader or other normal reader.

   > RapidShare Link

5. 10-27-2011, 04:13 PM #225
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > Code:

   >     extremely important message !!!

   >     seems most of lately produced msm7227-based phones have chipset with FIXED security hole, which used to altbypass unlock.
   >     ( that is not 100% confirmed, we only have few reports, however better be warned )
   >     such phones will DIE after successful unlock procedure.
   >     such dead phones CAN NOT be recovered. ( perhaps, jtag can fix that, perhaps, qualcomm fixed jtag security hole too )

   >     there is NO WAY to determine if phone has fixed chipset or chipset with security hole.

   >     the ONLY safe way is to use unlock by resurrection cables.
   >     if phone can be connected and booted by resurrection cables, phone is safe to unlock.
   >     if phone can not be booted by resurrection cables, phone has fixed chipset and could not be unlocked.

   >     you have been warned.
   >     get and use resurrection cables.

   > update:
   > Code:

   >     e16 phone with manufacture date 11w38 affected, i think we should care about phones which produced after 11w26

6. 11-05-2011, 11:50 AM #226
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v1.1202
   > Code:

   >     -  no testpoint altbypass unlock procedure will work now for msm7227-based phones,which using MCUs with fixed security bug.
   >        resurrection cables will NOT work for MCUs with fixed security bug. Because of this,
   >        phones, which are already dead should be recovered using jtag box, which can write ORIGINAL semc boot.
   >        big thanks for help and testing to electrolandgsm.
   >     -  switch to usb interface was broken for DB200x phones, fixed.
   >     -  added few models to list, so users can use profiles for them.

   > RapidShare Link

7. 12-09-2011, 04:21 PM #227
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > v1.1203
   > Code:

   >     -  testpoint altbypass method will work now for msm7227-based phones,which using MCUs with fixed security bug.
   >        that means, resurrection cables will work for MCUs with fixed security bug.
   >     -  fixed problem with FOTA upgrade for msm8x55-based phones, unlocked by altbypass

   > RapidShare Link

8. 12-24-2011, 07:52 PM #228
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > بِسْمِ اللّهِ الرَّحْمنِ الرَّحِيمِ
   > Starting from 25.12.2011 cost of unlock procedure, using alternative security bypass for semc phones,
   > based on msm7227,qsd8250,qsd8x55 chipsets will be 0 ( zero ) credits.
   > Such terms will be in effect until another announcement.

9. 01-02-2012, 08:05 PM #229
   the_laser
   - View Profile
   - View Forum Posts
   - Private Message
   Administrator

   Join Date
     Feb 2010
   Posts
     18,774

   ##

   > Holidays ended, time to work.
   > Starting from 03.01.2012 cost of unlock procedure, using alternative security bypass for semc phones,
   > based on msm7227,qsd8250,qsd8x55 chipsets will be 2 ( two ) credits.
   > we will watch closely on market situation with semc qualcomm solution and react correspondingly.

10. 03-29-2012, 11:14 AM #230
    the_laser
    - View Profile
    - View Forum Posts
    - Private Message
    Administrator

    Join Date
      Feb 2010
    Posts
      18,774

    ##

    > v1.1204
    > Code:

    >     - fixed "dead phone after unlock" for some latest j20 phones.
    >     - x10 with android firmware 2.3.3 supported for altbypass unlock
    >     - msm8x60 sony phones supported ( lt26,lt28,is12s,so-03d ). Standard operations supported - flash,trim area read/write.
    >       Network unlock only supported using s1 signature server, which is offline for us.
    >     - added support for one interesting activation.

    > RapidShare Link

Page 23 of 31 First ... 13 21 22 23 24 25 ... Last

- Jump to page:

Quick Navigation News & Updates Top

- Site Areas
- Settings
- Private Messages
- Subscriptions
- Who's Online
- Search Forums
- Forums Home
- Forums
- SETool2 Official support (English)
  1. News & Updates
  2. F.A.Q.
- HMD Tool Official support (English)
  1. News & Updates
- Other
  1. Offtopic & Trash

« Previous Thread | Next Thread »

#### Tags for this Thread

news, setool

View Tag Cloud

#### Bookmarks

- Digg
- Google
- del.icio.us
- StumbleUpon

#### Posting Permissions

- You may not post new threads
- You may not post replies
- You may not post attachments
- You may not edit your posts

- BB code is On
- Smilies are On
- [IMG] code is On
- [VIDEO] code is On
- HTML code is Off

Forum Rules