; platform.def
; (Rev. 0307221435)
;
; DO NOT change this file unless you really know what you are doing !!!
;

[Customer T: S10x]
BootLoader=passive
FlashLoader=fl_sceptre3_sgh_hw3_v24.sre

[Customer T: S20x, S30x, V20x]
BootLoader=passive
FlashLoader=fl_sceptre3_sgh_hw4_v24.sre

[Customer T: X40x]
BootLoader=passive
FlashLoader=fl_sceptre3_sgh_hw5_v24.sre

[Customer T: E71x, P720]
MIT=0
BootLoader=passive
SetupLoader=sl_sceptre3_nice_std.sre
SetupLoaderBaseAddr=0x04000000
FlashLoader=fl_sceptre3_nice_std_v24.sre
FlashLoaderBaseAddr=0x00000000
StackBaseAddr=0x00000000
ChipDesc=1
Flash0=0x00000000,16,0
Flash1=0x01000000,16,2

[Customer T: D418]
MIT=0
BootLoader=passive
SetupLoader=sl_sceptre3_nice_std.sre
SetupLoaderBaseAddr=0x04000000
FlashLoader=fl_sceptre3_nice_std_v24.sre
FlashLoaderBaseAddr=0x00000000
StackBaseAddr=0x00000000
ChipDesc=1
Flash0=0x00000000,16,0
Flash1=0x01000000,16,2

[Customer T: E308]
MIT=0
BootLoader=passive
SetupLoader=sl_sceptre3_nice_std.sre
SetupLoaderBaseAddr=0x04000000
FlashLoader=fl_sceptre3_nice_std_v24.sre
FlashLoaderBaseAddr=0x00000000
StackBaseAddr=0x00000000
ChipDesc=1
Flash0=0x00000000,16,0
Flash1=0x01000000,16,5

[Customer T: E608]
MIT=0
BootLoader=passive
SetupLoader=sl_sceptre3_nice_std.sre
SetupLoaderBaseAddr=0x04000000
FlashLoader=fl_sceptre3_nice_std_v24.sre
FlashLoaderBaseAddr=0x00000000
StackBaseAddr=0x00000000
ChipDesc=1
Flash0=0x00000000,16,0
Flash1=0x01000000,16,4

[Customer T: P720 (USB)]
MIT=0
BootLoader=passive
SetupLoaderIgnore=1
FlashLoader=fl_sceptre3_nice_std_usb.sre
FlashLoaderBaseAddr=0x00080000
StackBaseAddr=0x00000000
ChipDesc=1
Flash0=0x00000000,16,0
Flash1=0x01000000,16,2

[Customer T: P400]
MIT=0
BootLoader=passive
SetupLoader=sl_sceptre3_nice_std.sre
SetupLoaderBaseAddr=0x04000000
FlashLoader=fl_sceptre3_nice_std_v24.sre
FlashLoaderBaseAddr=0x00000000
StackBaseAddr=0x00000000
ChipDesc=1
Flash0=0x00000000,8,0
Flash1=0x00800000,8,5

[Customer T: P408, X438, X458]
MIT=0
BootLoader=passive
SetupLoader=sl_sceptre3_nice_std.sre
SetupLoaderBaseAddr=0x04000000
FlashLoader=fl_sceptre3_nice_std_v24.sre
FlashLoaderBaseAddr=0x00000000
StackBaseAddr=0x00000000
ChipDesc=1
Flash0=0x00000000,8,0
Flash1=0x00800000,8,2

[Customer T: S208, S308]
MIT=0
BootLoader=passive
SetupLoader=sl_sceptre3_nice_std.sre
SetupLoaderBaseAddr=0x04000000
FlashLoader=fl_sceptre3_nice_std_v24.sre
FlashLoaderBaseAddr=0x00000000
StackBaseAddr=0x00000000
ChipDesc=1
Flash0=0x00000000,8,0
Flash1=0x00800000,8,3

[Customer T: Edge flat board (UARTs 0/1)]
MIT=1
SetupLoader=sl_sceptre4_sgh_hw1.sre
SetupLoaderBaseAddr=0x00000000
FlashLoader=fl_sceptre4_sgh_hw1_v24.sre
FlashLoaderBaseAddr=0x24000000
StackBaseAddr=0x20000000
Flash0=0x20000000,8
Flash1=0x28000000,8

[Customer T: Edge flat board (UARTs 0/2)]
MIT=1
SetupLoader=sl_sceptre4_sgh_hw2.sre
SetupLoaderBaseAddr=0x00000000
FlashLoader=fl_sceptre4_sgh_hw2_v24.sre
FlashLoaderBaseAddr=0x24000000
StackBaseAddr=0x20000000
Flash0=0x20000000,8
Flash1=0x28000000,8

[Customer T: Edge flat board (USB)]
MIT=1
SetupLoaderIgnore=1
;SetupLoader=sl_sceptre4_sgh_hw2.sre
;SetupLoaderBaseAddr=0x00000000
FlashLoader=fl_sceptre4_sgh_hw2_usb.sre
;FlashLoaderBaseAddr=0x24000000
FlashLoaderBaseAddr=0x24080000
StackBaseAddr=0x20000000
Flash0=0x20000000,8
Flash1=0x28000000,8

