XDANDROID 2.2 AOSP
Main thread: http://forum.xda-developers.com/showthread.php?t=711692
Wiki: xdandroid.com
Facebook fan page: http://www.facebook.com/home.php?#!/pages/XDAndroid/394317262428
Twitter: http://twitter.com/xdandroid
Youtube channel: http://www.youtube.com/user/xdandroid

Please donate to the XDAndroid team :)
Every little bit counts and helps motivate us :p
http://xdandroid.com/w/donate.php


SELECT THE CORRECT STARTUP. 
COPY AND PASTE IT INTO THE ROOT OF ANDBOOT DIR. 
IF YOU ARE HAVING TROUBLE BOOTING. REMOVE "pmem.extra=1" FROM YOUR STARTUP.

Load XDANDROID within a custom named folder
Set Android directory: "rel_path=XXXXXXXX"
Set directory to where you are storing your installation
Eg: Put all files into folder named xdandroid
so cmd will be rel_path=xdandroid
Use this if you want to keep you SDcard more organised.

Waiting for SDCard error
For people who have problems with sdcard message, add this to your startup
msmsdcc_1bit msmsdcc_fmax=14000000 msmsdcc_nopwrsave

Turning on led flash
echo 1 > /sys/class/htc_hw/flash

Diamond Storage Issues (Storage Card Unmounted)

Startup|default configs options
Overclocking
acpuclock.oc_freq_khz=XXXXXX ( i personally use 600000-640000 )
but it very unstable if you try to get higher than 650000-700000

Physical Keyboard layout
physkeyboard=fuze
physkeyboard=raph
physkeyboard=nordic_raph
physkeyboard=tilt2
physkeyboard=rhod210
physkeyboard=rhod100_de
physkeyboard=rhod100_fr
physkeyboard=rhod100_it
physkeyboard=rhod100_uk
physkeyboard=rhod100_nordic
physkeyboard=rhod400
physkeyboard=rhod500
physkeyboard=swiss_raph
physkeyboard=german_raph

Button wake up
board-htcraphael-navi.wake=X 
0 = screen only wakes on power button
1 = wakes on any keypress

Onscreen terminal keyboard
msmvkeyb_toggle= (on/off)
on = displays terminal onscreen keyboard
off = hide terminal onscreen keyboard

Headset
snd.force_headset=X
1=USB headset
2=3.5mm headset

Incall volume adjust
htc_hw.call_vol=X
0-5
0: being lowest and 5: being loudest

Enable/Disable handsfree
htc_hw.handsfree=X
1=Enable
0=Disable

Recommended best loud and clear voice values are said to be 5/1
htc_hw.call_vol=5
htc_hw.handsfree=1

Disable low battery Warning
htc_battery_smem.fake=1 

Disable/Enable HW3d
hw3d.force=X
0=off
1=on 

LCD density / resolution
lcd.density=XXX
210 = 640x480 VGA devices
240 = 800x480 WVGA devices