#
# BT Patch Information File
# ====================================
#
# All patch file information must be stored as follows
#
# Philips:
# <CHIP_ID> <HCI_revision> <LMP_Subversion> <Patchfile>
#
# there CHIP_ID, HCI_revision and LMP_Subversion are read from firmware at start-up.
#
# ST: <CHIP_ID> is set to 0x00000000 since this is not used by ST.
#
# NOTE: From STE platform P1T and later <CHIP_ID> information shall not be listed!
#
# ====================================
# STLC2500_R4_02_A7.ptc                            patch for STLC2500C4 and STLC2590
# STLC2500_R5_01_A8.ptc                            patch for STLC2592
# STLC2500_R5_02_A1_E7.ptc                         patch for STLC2593 (2593 D2)
# STLC2500_R5_03_A12.ptc                           patch for STLC2593 (2593 D3)
# STLC2500_R5_04_A8.ptc                            patch for STLC2594 (2594)
# STLC2600_R6_00_A1_E6.ptc                         patch for STLC2690 (STLC2690 CUT 1)
# STLC2690_R6_03_A1_E5.ptc                         patch for STLC2690 (STLC2690 CUT 2.1)
# STLC2690_R6_04_A3_E3_CM00009835_TESTPATCH.ptc    patch for STLC2690 (STLC2690 CUT 3.0 CB10EG (LMP_Subversion 1D))
# STLC2690_R6_04_A3_E3_CM00009835_TESTPATCH.ptc    patch for STLC2690 (STLC2690 CUT 3.0 CB10EH (LMP_Subversion 1E))
# STLC2690_R6_05_A6.ptc                         patch for STLC2690 (STLC2690 CUT 4.0 (LMP_Subversion 1F))
# STLC2690_R6_05_A6.ptc                         patch for STLC2690 (STLC2690 CUT 4.1 (LMP_Subversion 2F))
# ----------------------------------------------------------------------------------------
0x0402  0x0520  STLC2500_R4_02_A7.ptc
0x0501  0x00EF  STLC2500_R5_01_A8.ptc
0x0502  0x00F0  STLC2500_R5_02_A1_E7.ptc
0x0503  0x00F1  STLC2500_R5_03_A12.ptc
0x0504  0x00F2  STLC2500_R5_04_A8.ptc
0x0600  0x0001  STLC2600_R6_00_A1_E6.ptc
0x0603  0x0014  STLC2690_R6_03_A1_E5.ptc
0x0604  0x001D  STLC2690_R6_04_A3_E3_CM00009835_TESTPATCH.ptc
0x0604  0x001E  STLC2690_R6_04_A3_E3_CM00009835_TESTPATCH.ptc
0x0605  0x001F  STLC2690_R6_05_A6.ptc
0x0605  0x002F  STLC2690_R6_05_A6.ptc
