##############################################################################################
#  ____                      _____      _                                                    #
# / ___|  ___  _ __  _   _  | ____|_ __(_) ___ ___ ___  ___  _ __                            # 
# \___ \ / _ \| '_ \| | | | |  _| | '__| |/ __/ __/ __|/ _ \| '_ \                           # 
#  ___) | (_) | | | | |_| | | |___| |  | | (__\__ \__ \ (_) | | | |                          # 
# |____/ \___/|_| |_|\__, | |_____|_|  |_|\___|___/___/\___/|_| |_|                          # 
#                    |___/                                                                   # 
#                                                                                            #      
# Version Compact Camera Manager Settings™  for w995                                         #   
# Optimized for the Sony Ericsson w995                                                       # 
##############################################################################################
# Copyright® 2010 Sony Ericsson Mobile Communications.                                       #
# All rights, including trade secret rights, reserved.                                       #
# BrAzzUkA's TEAM BZK® Camera Drivers respects the intellectual property of others,          #
# and we ask our modders and users to do the same.                                           #
##############################################################################################
// Visit the website: 
//http://forums.se-nse.net/topic/43199-jocks-extreme-sharpness%E2%84%A2-14-special-edition%E2%84%A2-for-w995
//http://www.esato.com/board/viewtopic.php?topic=191301


About Compact Camera Manager Settings™:
---------------------------------------
Compact Camera Manager Settings™ The logical device is implemented enough for you to control all the functions that a semi pro camera has. 
Manual settings is a different approach to manage camera parameters by included additional functionality layer 
and every logical programming which is not available in original driver.You decide when you turn on or turn off the manual settings for your cam.
The manual settings for this models is worked to optimize the functions and not waste other necessary functions, this is the manual settings is optimized to work in any condition with flash *xenon flash or without flash, and all functions work together with their steps and settings.The keys to the steps are the same for reasons obvious, then we can use the controller EV to the steps 
Compact Camera Manager Settings™ is an additional layer of functionality which is not available in original driver.
This layer collects many manual functions which makes you able to control parameters yourselfand not rely only on point & shoot automatic settings.
You can use the Compact Camera Manager Settings™ in automatic mode, the camera is still good POINT AND SHOT solution
Compact Camera Manager Settings™ is as simple as point and shoot camera is due to them having more settings to learn to use Once you have a good feel for settings Automatic Compact Camera Manager Settings™ you can start
learn to use manual settings and add the extras. Manual configuration to give you total control over his photography and style of images you take.

Note 1: This driver works on any compatible only mobile phone model w995 with any version of cam module.
Note 2: This manual describes driver with default settings.
Note 3: You can change all settings in the cuztomize scenes section of the driver.
Note 4: This manual describes driver with default settings. 
Note 5: You can change all settings in the Config section of the driver. 
Note 6: Manual settings simple where the user can choose to enable or disable the manual settings. 
Note 7: Camdriver optimized for implementation of manual settings. 
Note 8: No patches or graphical interfaces only if the user want. 



Menu scenes = Menu functions manual settings Compact Camera Manager Settings™
-----------------------------------------------------------------------------
Auto => ISO
Portrait => Shutter Speed slow/fast
Landscape => Focus
Night (Twilight portrait) => Colors Saturation
Night Portrait (Twilight landscape) => Brightness
Beach & Snow => Contrast
Sports => Sharpness
Document => HUE

Now Scenes has the feature manual settings with all functions available working together.


Menu Effects= Menu Photo Mode = Scenes  /Menu Video Mode  Manual Settings for video
-----------------------------------------------------------------------------------

photo mode = scenes 

photo:
-----
Normal => Normal         
black and white => Portrait        
negative => Landscape       
sepia => Night        
Solarize => Sports   

*the effects on photo mode were replaced by scenes


video mode = manual settings for video

video:
------
Video => effects
Normal => off end end
black and white => color filter1
negative => color filter2
sepia => manual focus
Solarize => manual contrast

*the effects on video mode were replaced by manual settings video mode

Custom Video Movie Size
------------------------
//Video Movie Size Video resolution      
//"User"and "Modder"here you can change the resolution of the video in normal mode or night mode but remember to always test , use for this hex calc
//Find this lines below

//Video Movie Size Format support:
//[xx,yy,zz]      // xx=HL yy=VL zz=FPS
//[140,F0,BB8]    // VR  QVGA   320 x 240
//[160,120,BB8]   // VR  CIF    352 x 288
//[190,F0,BB8]    // VR  WQVGA  400 x 240
//[280,1E0,BB8]   // VR  VGA    640 x 480

Video:
======
Two [2] Resolutions for video recording Two [2] Movie Size
You can use the video with the manual settings for video

Movie Size: 
-QVGA 320x240 Normal video recording 25fps to 30fps [QVGA] 
-CIF 352x288 video recording 15fps to 25fps 
Access the Menu Mode Night or Mode Video:
-To video recording in normal video resolution 320x240 , just switch to video mode Normal Mode (disable Nigth Mode) or Normal resolution 320x240.
-To video recording in CIF resolution 352x288 , turn Nigth Mode resolution 352x288. 



How to use this camdriver Compact Camera Manager Settings™:
============================================================
It's very easy, it's actually original camdriver + some manual settings.
you can lock your favourite settings and take the pic. you can change shutter Spedd, ISO,Saturation, Sharpness, Contrast, Brightness, Hue, *Colors Correction, Color Filters, Focus, Effects. also if you lock ISO you can change
*Colors Correction = Color Filters
With Compact Camera Manager Settings™ all the functions work together and with that all the settings changed by the user are accumulated, you can move each function to your liking and set to either manual adjustments.
You can set every function at a time as ISO, Shutter Speed slow/fast, Colors Saturation, Colors Correction WB or Filter Colors, Contrast, Brightness, Sharpness, HUE, Focus, Effects etc...
You can also use the manual settings only for video with your Compact Camera Manager Settings™.
Photo mode and Video mode are separate so you can make better use.
Restart the camera functions back to default.



Controller Compact Camera Manager Settings™:
============================================
- Changing EV:
   This  function is optimized to be used when the Camera Manager Settings™ is turn [off], you use the EV settings normally,with joypad you can change EV.
	
- Changing Saturation:
    In menu choose Manual Settings, choose 'Saturation', with joypad you can change Saturation (just like changing EV).

- Changing Sharpness:
    In menu choose Manual Settings, choose 'Sharpness', with joypad you can change Sharpness (just like changing EV).

- Changing ISO:
    In menu choose Manual Settings, choose 'ISO', with joypad you can change ISO (just like changing EV)

- Changing Shutter Speed slow/fast:
    In menu choose Manual Settings, choose 'Shutter Speed', with joypad you can change Shutter Speed (just like changing EV)

- Changing Shutter Speed LED Flash slow/fast:
    This  function is optimized to be used when the LED flash is turn [on], you use the shutter speed xenon flash settings normally, with joypad you can change EV.
    The function ISO LED Flash work together with shutter Speed LED Flash.

- Changing ISO LED Flash:
    The function ISO Xenon Flash work together with shutter Speed Xenon Flash.

- Changing Contrast:
    In menu choose Manual Settings, choose 'Contrast', with joypad you can change Contrast (just like changing EV)

- Changing Brightness:
    In menu choose Manual Settings, choose 'Brightness', with joypad you can change ISO (just like changing EV)

- Changing HUE:
    In menu choose Manual Settings, choose 'HUE', with joypad you can change HUE (just like changing EV)

- Changing Colors Correction = Color Filters:
    In menu choose Manual Settings, choose 'Colors Correction = Color Filters', with joypad you can change Color Filters1 and Color Filters2 (just like changing EV)

- Changing Effects:
    In menu choose Manual Settings, choose 'Effects', with joypad you can change Effects (just like changing EV). Implemented more than 5 effects for you user.
    *Special Effects

- Changing Focus:
    In menu choose Manual Settings, choose 'Focus', with joypad you can change Focus (just like changing EV).



Instructions for change LNG Interface:
-------------------------------------
The driver must be installed in this folder:

IFS \ SETTINGS \ CAMERA

Delete the file "camdriver0.dat" and "camdriver1.dat" and drag and drop the file Unpack with the same names (CAN NOT BE DIFFERENT NAME).

camdriver0.dat=> for camera
camdriver1.dat=> for frontal camera or video call

Files *. lng (language)
Should be placed in this folder:

TPA \ PRESET \ SYSTEM \ LANGUAGE

Drag and drop the files "pb.lng" and "en.lng" "de.lng" "sv.lng" folder above.

How to change *.lng:

    - Download LngEditor
    - you will need .NET FrameWork 2.0 to run it. you can download it from Microsoft website.
    - Download your current FS from 4shared
    - Follow this guide to extract FS.
    - Find *.lng file you want to edit in TPA\PRESET\SYSTEM\LANGUAGE
    - Open the file with LngEditor and edit it, then save it.



//   ########                    #####
//  ###########              ####     ##
//   ###########           ###        # 
//   #############        ##            
//   ##############     ##              
//   ###############   ##               
//    ############### ##                
//     ################                 
//         #        ############        
//      #           ###############     
//     #           #################    
//     #          ##################    
//     ##         ##  ##############    
//      #  ©2010 ##    ###BZK®™#####    
//       ##  #  ##      ##########      
//         #####          ######
// Sony Ericsson CameraDrivers BrAzzUkA's Team BZK®
//
//Programming Software Sensor Camera License Agreement:
//The CameraDrivers BrAzzUkA's Team BZK® grants you a limited licence to use the codes of the sensors camera and the codes of the sensors second camera embedded in this driver "the Software" in binary and hexadecimal executable form in the normal operation of the driver. Title ownership rights and intellectual property rights and Logic Programming and Programming Sensors remain in CameraDrivers BrAzzUkA's Team BZK®.
//You acknowledge that Logic Programming and Programming Sensors is the property of CameraDrivers BrAzzUkA's Team BZK® and the codes of sensors is property Sony Ericsson and partner companies in the manufacture of sensors is protected under the Software License Agreement copyright laws and international copyright treaties. You further acknowledge that the structure, organization and codes programming sensors are avaliable trade secrets of CameraDrivers BrAzzUkA's Team BZK®.
//You agree not to decompile, disassemble, modifiy,reverse assemble, reverse engineer or reduce to human readable form the programming or any part of scheme or any part thereof or create any derivative works based on the programmin sensor or scheme CameraDrivers BrAzzUkA's Team BZK®.
//You agree not to export or re export, not copy or edit the programming sensor and schemma to any country or other vehicle communication in violation of the export control laws International.You agree not to sell the programming of sensor camera and the drivers in any hypothesis, that you and is explicit which may in no circumstances shall the sale of the drivers for profit under the law as the copyright.
//The information and codes published in camdrivers are available to any modders and user, 
//but may not necessarily be copied, downloaded or reused,reproduced without credit to the developers.
//Thanks and respect the developers. :)
